*************************** START ****************************

START TIME: 202302091218

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xc6836bcc
mac h: 0x6e943c
crc_cal: 110
crc_read: 110
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600200
Update flash status done!

Wrote 835168 bytes (478716 compressed) at 0x00010000 in 8.0 seconds (effective 830.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



