*************************** START ****************************

START TIME: 202304271002

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x7e498bdc
mac h: 0xf80cdc
crc_cal: 248
crc_read: 248
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600200
Update flash status done!

Wrote 808272 bytes (516561 compressed) at 0x00010000 in 8.3 seconds (effective 779.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



