*************************** START ****************************

START TIME: 202301251157

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xcd929db4
mac h: 0x1be831
crc_cal: 27
crc_read: 27
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600200
Update flash status done!

Wrote 805632 bytes (518841 compressed) at 0x00010000 in 9.2 seconds (effective 704.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202301251253

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xcd929db4
mac h: 0x1be831
crc_cal: 27
crc_read: 27
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!

Wrote 805792 bytes (518974 compressed) at 0x00010000 in 9.1 seconds (effective 707.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202301251255

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xcd929db4
mac h: 0x1be831
crc_cal: 27
crc_read: 27
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!

Wrote 805792 bytes (518974 compressed) at 0x00010000 in 9.2 seconds (effective 701.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202301251257

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xcd929db4
mac h: 0x1be831
crc_cal: 27
crc_read: 27
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!

Wrote 805792 bytes (518974 compressed) at 0x00010000 in 9.1 seconds (effective 706.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



